

Standard Features

***5 WIDE SINGLE AXLES***

24” o.c. Cross Members White Alum. Metal White Spoke Wheels 2990# Drop Dexter Axle

24” o.c. Roof Members Screwed Exterior St 205 15” Radial Tires E-Z Lube Hubs

16” o.c. Side Wall Posts Interior Height 60’ Alum. Jeep Style Fenders Flat 4 Way Elect. Plug

2000# A-Frame Jack 3/4” Plywood Floors Galvalume Roof Single Swing Rear Door

2” Coupler 3/8” Plywood Walls Non Powered Roof Vent Round Top W/Fiberglass Cap

3” Steel Tube Main Frame 1-12volt Dome Lite 24” ATP Stone Guard LED lights through-out

***6 & 7 WIDE SINGLE AXLES***

24” o.c. Cross Members White Alum. Metal White Spoke Wheels 2990# Drop Dexter Axle

24” o.c. Roof Members Screwed Exterior St 205 15” Radial Tires E-Z Lube Hubs

16” o.c. Side Wall Posts Interior Height 72” Alum. Jeep Style Fenders Flat 4 Way Elect. Plug

2000# A-Frame Jack 3/4” Plywood Floors Galvalume Roof Double Rear Door

2” Coupler 3/8” Plywood Walls Non Powered Roof Vent Round Top W/Fiberglass Cap

3” Steel Tube Main Frame 1-12volt Dome Lite 24” ATP Stone Guard LED lights Through-out

32” Side Door w/bar lock Door Hold Back latch

***6 & 7 WIDE TANDEM AXLES***

24” o.c. Cross Members White Alum. Metal White Spoke Wheels 2-3500# Drop Dexter Axles

24” o.c. Roof Members Screwed Exterior St 205 15” Radials Tires E-Z Lube Hubs

16” o.c. Side Wall Posts Interior Height 72” Smooth Alum. Fenders Round 7 Way Elect. Plug

2000# A-Frame Jack 3/4” Plywood Floors Galvalume Roof Double Rear Door

2 5/16” Coupler 3/8” Plywood Walls Non Powered Roof Vent Round Top W/Fiberglass Cap

4” Steel Tube Main Frame 1-12volt Dome Lite 24” ATP Stone Guard LED lights Through-out

(6” Frame 16’ or longer) 32” Side Door w/bar Door Hold Back latch Elect. Brakes both Axles

***8 & 8.5 WIDE***

16” o.c. Cross Members White Alum. Metal White Spoke Wheels 2-3500# Drop Dexter Axles

24” o.c. Roof Members Screwed Exterior St 205 15” Radial Tires E-Z Lube Hubs

16” o.c. Side Wall Posts Interior Height 78” Smooth Alum. Fenders Round 7 Way Elect. Plug

2000# A-Frame Jack 3/4” Plywood Floors Galvalume Roof Double Rear Door (8’ wide)

2 5/16” Coupler 3/8” Plywood Walls Non Powered Roof Vent Anodized Front Corners

6” Steel I-Beam Frame 1-12volt Dome Lite 24” ATP Stone Guard LED lights through-out

36” Side Door w/bar Door Hold Back latch Elect. Brakes both Axles Flat Top Roof

*(8.5 Wide include Heavy duty Rear Ramp w/16” Flap, Beaver Tail, 4-Floor D-rings, Anodized Front Corners)*

*(8.5 Wide Car Haulers 26’ or longer have 8” main frame and a 1-piece Alum. Roof)*